
[](https://www.google.com/url?sa=i&rct=j&q=&esrc=s&source=images&cd=&cad=rja&uact=8&ved=2ahUKEwj83ezu4r7gAhUxwcQHHQjcDsQQjRx6BAgBEAU&url=https%3A%2F%2Fracesport.carjamz.com%2F&psig=AOvVaw1ULlQ323dOfVo4918gaqT7&ust=1550355610607208)

**RSJL1804-JEEP JL Blacked Out Series LED Fog Light Kit**



1. **Begin by removing rear cover from behind the bumper, to get access to fog light assembly.**

1. **Once you have access to the fog light assembly you may remove the assembly by removing 3 bolts. They consist of a hex head bolt and a nut on the other side.**



1. **Once the assembly is off you may replace it with the new assembly and fog light with the factory bolts.**



1. **When the assembly is in its place you may make, your connections. Test polarity with a multimeter solder and shrink wrap you’re connections to the appropriate locations zip tie access wire so that it will not hang and get snagged on anything.**



1. **When connections are made and secured you may adjust light the fog light to preferred height by using the adjuster screw on the back of the assembly and enjoy.**



**If any questions, please feel free to contact us at tech service @ 847-327-0073 ext. 3**